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Peter Wolters AC 1200 configuration

· refurbished and upgraded with a modern Siemens control system


Description
· Double Disc Polishing Machine
· Condition: Completely refurbished
· Working disc diameter: Ø 1,200 mm
· Carrier drive system: 120 T 36/7
· Motor-driven outer pin ring
· New Siemens S7-315 PLC control
· New electrical control cabinet
· New Siemens HMI 1500 operator panel
· Three new frequency converters for all servo drives
· New electronic precision control
· Complete new pneumatic system
· Highly sensitive pneumatic working pressure control
· Automatic stepless pressure build-up
· Four independently adjustable pressure levels per processing cycle
· Infinitely adjustable pressure and speed ramps
· Program memory with 60 storage locations
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